PM-2 50UA Test Procedure：

1. Test “Zero” position



1. The balance test at 45degree, horizontal and vertical



3、Test the scale between Zero and full scale



1. Test at full scale



